[InitialSettings]
InstallerVersion=V5
CompanyNameReadme=SHARP
Driver=3
Driver_1=PCL6
Driver_2=PS
Driver_3=PPD
SearchMethodDefault=2
Advanced_Inst=ON
StartmenuName=
StartmenuName_Del1=
IFaxModelNumber=
NO_SEARCH_MODEL=OFF
PortMonitorIPP=scprint
DisableUpdateDialog=N
ArgDisableUpdateDialog=SETIP,USB SILENT,NETWORKSTD

[Model]
UNINST_KEY=SHARP Driver Uninstall Tool
UNINST_DISP_NAME=SHARP Driver Uninstall Tool
UNINST_VERSION=1.0.0.0
UNINST_PUBLISHER=SHARP CORPORATION

[ModelName]
nModelNum=11
Model1=MX-B4083D,Mono,40
Model2=MX-B5083D,Mono,50
Model3=MX-B6083D,Mono,60
Model4=SF-S502D,Mono,50
Model5=SF-S602D,Mono,60
Model6=MX-B4053R,Mono,40
Model7=MX-B5053R,Mono,50
Model8=MX-B6053R,Mono,60
Model9=SF-S352R,Mono,35
Model10=SF-S402R,Mono,40
Model11=SF-S502R,Mono,50

[USBID]
MX-B4083D=VID_04DD&PID_9EC5
MX-B5083D=VID_04DD&PID_9EC6
MX-B6083D=VID_04DD&PID_9EC7
SF-S502D=VID_04DD&PID_9ECB
SF-S602D=VID_04DD&PID_9ECC
MX-B4053R=VID_04DD&PID_9EC8
MX-B5053R=VID_04DD&PID_9EC9
MX-B6053R=VID_04DD&PID_9ECA
SF-S352R=VID_04DD&PID_9ECD
SF-S402R=VID_04DD&PID_9ECE
SF-S502R=VID_04DD&PID_9ECF

[ModelType]
ModelType=ON
MX-B4083D=4
MX-B5083D=4
MX-B6083D=4
SF-S502D=4
SF-S602D=4
MX-B4053R=1
MX-B5053R=1
MX-B6053R=1
SF-S352R=1
SF-S402R=1
SF-S502R=1


[Install]
README_DIR=MX3071PCLPS
EnableAutoConfigCheckBox=ON
DefaultRunAutoConfig=ON
NETWORK_SUPPORT=ON
LOCAL_CONNECTION=ON
USB_SUPPORT=OFF
TANDEM_SUPPORT=ON
IPP_SUPPORT=ON
FONT_SUPPORT=ON
FONT_INSTALL=ON
