[InitialSettings]
InstallerVersion=V5
CompanyNameReadme=SHARP
Driver=3
Driver_1=PCL6
Driver_2=PS
Driver_3=PPD
SearchMethodDefault=2
Advanced_Inst=ON
StartmenuName=
IFaxModelNumber=
NO_SEARCH_MODEL=OFF
PortMonitorIPP=scprint
DisableUpdateDialog=N
ArgDisableUpdateDialog=SETIP,USB SILENT,NETWORKSTD

[Model]
UNINST_KEY=SHARP Driver Uninstall Tool
UNINST_DISP_NAME=SHARP Driver Uninstall Tool
UNINST_VERSION=1.0.0.0
UNINST_PUBLISHER=SHARP CORPORATION

[ModelName]
nModelNum=4
Model1=MX-B6581D,Mono,65
Model2=MX-B7581D,Mono,75
Model3=SF-S651D,Mono,65
Model4=SF-S751D,Mono,75

[USBID]
MX-B6581D=VID_04DD&PID_9D27
MX-B7581D=VID_04DD&PID_9D28
SF-S651D=VID_04DD&PID_9D29
SF-S751D=VID_04DD&PID_9D2A

[ModelType]
ModelType=ON
MX-3070N=4
MX-3570N=4
MX-4070N=4
MX-3060N=4
MX-3560N=4
MX-4060N=4
MX-3050N=1
MX-3550N=1
MX-4050N=1
MX-5070N=4
MX-6070N=4
MX-5050N=1
MX-6050N=1
MX-M905=4
MX-6580N=4
MX-7580N=4
MX-2630N=1
MX-M5070=4
MX-M6070=4
MX-M5050=1
MX-M6050=1
MX-M3070=4
MX-M3570=4
MX-M4070=4
MX-M3050=1
MX-M3550=1
MX-M4050=1
MX-8090N=4
MX-7090N=4
MX-3060V=4
MX-3070V=4
MX-3560V=4
MX-3570V=4
MX-4060V=4
MX-4070V=4
MX-5070V=4
MX-6070V=4
MX-3050V=1
MX-3550V=1
MX-4050V=1
MX-5050V=1
MX-6050V=1
MX-B355W=4
MX-B455W=4
MX-M2630=1
MX-B350W=4
MX-B450W=4
MX-B350P=4
MX-B450P=4
MX-M6570=4
MX-M7570=4
AR-B351=4
AR-B451=4
MX-B351P=4
MX-B451P=4
AR-B353P=4
AR-B453P=4
MX-B350F=4
MX-B450F=4
AR-B351F=4
AR-B451F=4
MX-B350=4
MX-B450=4
AR-B351W=4
AR-B451W=4
AR-B352P=4
AR-B452P=4

[Install]
README_DIR=MX303540PCLPS
EnableAutoConfigCheckBox=ON
DefaultRunAutoConfig=ON
NETWORK_SUPPORT=ON
LOCAL_CONNECTION=ON
USB_SUPPORT=OFF
TANDEM_SUPPORT=ON
IPP_SUPPORT=ON
FONT_SUPPORT=ON
FONT_INSTALL=ON
